

***Data Line Protector Model:WT145RJI***

# APPLICATIONS:

* CAT5e and CAT5 compatible
* 10/100 Base-T Ethernet protection
* LAN, FDDI，CDDI, ATM
* PDH, SDH, SPDH
* Industrial control

# FEATURES:

* Multi. Protection circuits, Gas-Tube+ TVS technology
* Dual protection in Common mode and differential mode
* TVS array technology, low capacitance
* Multi-Strike Capability

# TECHNICAL PARAMETER：

Model WT150RJ Electrical Parameter

Max. continuous operating voltage Uc 5V ,Nominal discharge current（8/20µs）In 3kA Max. discharge current （8/20µs）Imax 5Ka Limiting voltage (10/700µs) Up

Line-line 25V Line-ground 500V

Adapt transmission rate 100Mbps Insertion loss 0.5dB Protection line 1/2, 3/6 Response time tA 1ns Interface form RJ45

Protection way 2

Protection port 1 Mechanical characteristics

Dimension 83(L) ×25(W) ×25(H)mm Weight per unit 76g IP Code IP20

Working conditions Temperature: -40 to 80℃, Relative humidity: ≤95％

Standards Compliance IEC61643-1, RoHS

**Welltech Enterprises**

415 Ground Floor, PRAKASH MOHALLA, GARHI , EAST OF KAILASH

NEW DELHI 110065

Phone +91 9871650366 Email : sales@welltechenterprises.in